; CANODR205.INF  -- Canon DR-2050C Setup File for x64
; Copyright (c) 2006 Canon Electronics Inc.

[Version]
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Provider%
DriverVer=07/27/2006,1.2.0.4
Catalogfile=CANODR205.cat

[DestinationDirs]
DefaultDestDir=11				; Win95,Win98 = \windows\system.  NT5 = \windows\system32

[Manufacturer]
%Mfg%=Models,NTamd64

[Models.NTamd64]
%CANON.USBDeviceDesc% = USB_SCANNER.NTamd64,USB\VID_04a9&PID_160A


; ********** USB Section **********

; 64bit section
[USB_SCANNER.NTamd64]
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=USB_SCAN.Events.NTamd64
DeviceData=USB_SCAN.DeviceData.NTamd64
AddReg=Usb.Scanner.AddReg.NTamd64
PropertyPages="CaDRcpl.dll,EnumStiPropPages"
ICMProfiles="sRGB Color Space Profile.icm"

[USB_SCAN.DeviceData.NTamd64]
TwainDS="Canon DR-2050C TWAIN"
ISISDriverName="DR2080C.PXN"
Model=%CANON.USBDeviceDesc%
QueryNotification="DR2KSVC.DLL"

[USB_SCAN.Events.NTamd64]
ScanButton="Scan Button",{829A2E38-0F27-4389-A8A5-7735A76D9485},%LaunchApplication%
JobStartButton="Job Tool",{F31C13A8-0801-4c6c-A17A-8174F25017EF},%LaunchJobApplication%

[USB_SCANNER.NTamd64.Services]
Include=sti.inf
Needs=STI.USBSection.Services


; ********** Model-Generic add registry Section **********

; 64bit USB add registry section
[Usb.Scanner.AddReg.NTamd64]
HKR,,HardwareConfig,1,4
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{DFDB3FF3-A518-4145-A404-D2C731EC4D63}"
HKCR,CLSID\{DFDB3FF3-A518-4145-A404-D2C731EC4D63},,,"Canon CeiUSB64"
HKCR,CLSID\{DFDB3FF3-A518-4145-A404-D2C731EC4D63}\InProcServer32,,,%11%\ceiusb64.dll
HKCR,CLSID\{DFDB3FF3-A518-4145-A404-D2C731EC4D63}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"usbscan.sys"


; ********** Strings **********

[Strings]
Provider="Canon Electronics Inc."
Mfg="CANON"
CANON.USBDeviceDesc="CANON DR-2050C USB"
LaunchApplication="*"
LaunchJobApplication="DR-2050C Job Tool"
