; CANODR2K.INF  -- Canon DR-2080C Setup File for x64
; Copyright (c) 2006 Canon Electronics Inc.

[Version]
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Provider%
DriverVer=07/27/2006,1.2.0.4
Catalogfile=CANODR2K.cat

[DestinationDirs]
DefaultDestDir=11				; Win95,Win98 = \windows\system.  NT5 = \windows\system32

[Manufacturer]
%Mfg%=Models,NTamd64

[Models.NTamd64]
%CANON.SCSIDeviceDesc% = SCSI_SCANNER.NTamd64,CANON___DR-2080C________0
%CANON.SCSIDeviceDesc% = SCSI_SCANNER.NTamd64,CANON___DR-2080C________1
%CANON.SCSIDeviceDesc% = SCSI_SCANNER.NTamd64,CANON___DR-2080C________2
%CANON.SCSIDeviceDesc% = SCSI_SCANNER.NTamd64,CANON___DR-2080C________3
%CANON.USBDeviceDesc% = USB_SCANNER.NTamd64,USB\VID_04a9&PID_1601


; ********** USB Section **********

; 64bit model section
[USB_SCANNER.NTamd64]
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=USB_SCAN.Events.NTamd64
DeviceData=USB_SCAN.DeviceData.NTamd64
AddReg=Usb.Scanner.AddReg.NTamd64
PropertyPages="CaDRcpl.dll,EnumStiPropPages"
ICMProfiles="sRGB Color Space Profile.icm"

[USB_SCAN.DeviceData.NTamd64]
TwainDS="Canon DR-2080C TWAIN"
ISISDriverName="DR2080C.PXN"
Model=%CANON.USBDeviceDesc%
QueryNotification="DR2KSVC.DLL"

[USB_SCAN.Events.NTamd64]
ScanButton="Scan Button",{829A2E38-0F27-4389-A8A5-7735A76D9485},%LaunchApplication%

[USB_SCANNER.NTamd64.Services]
Include=sti.inf
Needs=STI.USBSection.Services


; ********** SCSI sections **********

; 64bit model section
[SCSI_SCANNER.NTamd64]
Include=sti.inf
Needs=STI.SCSISection
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=SCSI_SCAN.Events.NTamd64
DeviceData=SCSI_SCAN.DeviceData.NTamd64
AddReg=Scsi.Scanner.AddReg.NTamd64
PropertyPages="CaDRcpl.dll,EnumStiPropPages"
DeviceSubType=0x0101
ICMProfiles="sRGB Color Space Profile.icm"

[SCSI_SCAN.DeviceData.NTamd64]
TwainDS="Canon DR-2080C TWAIN"
ISISDriverName="DR2080C.PXN"
Model=%CANON.SCSIDeviceDesc%
QueryNotification="DR2KSVC.DLL"

[SCSI_SCAN.Events.NTamd64]
ScanButton="Scan Button",{829A2E38-0F27-4389-A8A5-7735A76D9485}, %LaunchApplication%

[SCSI_SCANNER.NTamd64.Services]
Include=sti.inf
Needs=STI.SCSISection.Services


; ********** Model-Generic add registry Section **********

; 64bit SCSI add registry section
[Scsi.Scanner.AddReg.NTamd64]
HKR,,HardwareConfig,1,2
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{7222EC61-956A-4bcf-B8D2-99A90B167594}"
HKCR,CLSID\{7222EC61-956A-4bcf-B8D2-99A90B167594},,,"Canon CeiSCSI64"
HKCR,CLSID\{7222EC61-956A-4bcf-B8D2-99A90B167594}\InProcServer32,,,%11%\ceiscs64.dll
HKCR,CLSID\{7222EC61-956A-4bcf-B8D2-99A90B167594}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"scsimap.sys,scsiscan.sys"

; 64bit USB add registry section
[Usb.Scanner.AddReg.NTamd64]
HKR,,HardwareConfig,1,4
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{DFDB3FF3-A518-4145-A404-D2C731EC4D63}"
HKCR,CLSID\{DFDB3FF3-A518-4145-A404-D2C731EC4D63},,,"Canon CeiUSB64"
HKCR,CLSID\{DFDB3FF3-A518-4145-A404-D2C731EC4D63}\InProcServer32,,,%11%\ceiusb64.dll
HKCR,CLSID\{DFDB3FF3-A518-4145-A404-D2C731EC4D63}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"usbscan.sys"


; ********** Strings **********

[Strings]
Provider="Canon Electronics Inc."
Mfg="CANON"
CANON.SCSIDeviceDesc="CANON DR-2080C SCSI"
CANON.USBDeviceDesc="CANON DR-2080C USB"
CANON.UsdName="CANON DR-2080C USD"
LaunchApplication="CapturePerfect"
