[Version]
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Provider%
DriverVer=11/18/2005,1.2.0.7

[DestinationDirs]
DefaultDestDir=11				; Win95,Win98 = \windows\system.  NT5 = \windows\system32
Usb.Scanner.CopySys32Files=10,system32\drivers  ; \windows\system32\drivers

[Manufacturer]
%Mfg%=Models

[Models]
%CANON.USBDeviceDesc% = USB_SCANNER,USB\VID_04a9&PID_1608


; ********** USB Section **********

; Win98 model section
[USB_SCANNER]
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=USB_SCAN.Events
DeviceData=USB_SCAN.DeviceData
AddReg=Usb.Scanner.AddReg
CopyFiles=Usb.Scanner.CopyFiles,Usb.Scanner.CopySys32Files
PropertyPages="DR25CPL.dll,EnumStiPropPages"
;DeviceSubType=0x0105
ICMProfiles="sRGB Color Space Profile.icm"

; Win2000 model section
[USB_SCANNER.NT]
Include=sti.inf
Needs=STI.USBSection

SubClass=StillImage
DeviceType=1
Capabilities=3
Events=USB_SCAN.Events
DeviceData=USB_SCAN.DeviceData
AddReg=Usb.Scanner.AddReg.NT
CopyFiles=Usb.Scanner.CopyFiles.NT
PropertyPages="DR25CPL.dll,EnumStiPropPages"
;DeviceSubType=0x0105
;VendorSetup="Dr25svc.dll,EntryPointInst"
ICMProfiles="sRGB Color Space Profile.icm"

[USB_SCAN.DeviceData]
ISISDriverName="DR2580C.PXN"
TwainDS="Canon DR-2580C TWAIN"
Model=%CANON.USBDeviceDesc%
QueryNotification="DR25SVC.DLL"

[USB_SCAN.Events]
;GreenButton=%GreenButton%,{AD879F40-0982-11d1-A43B-080009EEBDF6},*
;CopyButton=%CopyButton%,{B38E1061-65AB-11d1-A43B-080009EEBDF6},HP ScanJet Copy Utility
;ScanButton="Scan Button",{829A2E38-0F27-4389-A8A5-7735A76D9485},%LaunchApplication%
Button1="Button No.1",{EA2C292C-2416-4367-A29D-C086B84441F6},%LaunchApplication%
Button2="Button No.2",{A21D8598-94AA-4e37-B336-709EF0F1BF9A},%LaunchApplication%
Button3="Button No.3",{C1900B9E-E9FA-4710-A7E9-579E667639F7},%LaunchApplication%
JobStartButton="Job Tool",{96678965-3E4B-4467-AEA3-DF0ECB53BD28},%LaunchJobApplication%

[USB_SCANNER.NT.Services]
Include=sti.inf
Needs=STI.USBSection.Services


; ********** Model-Generic add registry and copy Section **********

; Win98 USB add registry section
[Usb.Scanner.AddReg]
HKR,,HardwareConfig,1,4
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{42B08D3F-3AC2-43c4-9455-E8264B18EB80}"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80},,,"Canon CeiUSB2"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,,,%11%\ceiusb2.dll
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"usbscan.sys"

; Win2000 USB add registry section
[Usb.Scanner.AddReg.NT]
HKR,,HardwareConfig,1,4
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{42B08D3F-3AC2-43c4-9455-E8264B18EB80}"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80},,,"Canon CeiUSB2"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,,,%11%\ceiusb2.dll
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"usbscan.sys"

; Win98 copy files section
[Usb.Scanner.CopyFiles]

; Win2000 copy files section
[Usb.Scanner.CopyFiles.NT]

; Only used by Win98
[Usb.Scanner.CopySys32Files]


; ********** Source Disk Section **********

; the number is used in the SourceDisksFiles section
[SourceDisksNames]
; testing, change path below to path on media
1=%Disk Name%,,

; the number maps to the SourceDisksNames number
[SourceDisksFiles]

; ********** Strings **********

[Strings]
Provider="Canon Electronics Inc."
Mfg="CANON"
Disk Name="CANON DR-2580C Driver Disk"
CANON.USBDeviceDesc="CANON DR-2580C USB"
LaunchApplication=*
LaunchJobApplication="DR-2580C Job Tool"


