[Version]
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Provider%
DriverVer=11/18/2008,1.0.0.0
CatalogFile=CANONDR905.cat

[DestinationDirs]
DefaultDestDir=11				; Win95,Win98 = \windows\system.  NT5 = \windows\system32

[Manufacturer]
%Mfg%=Models,NTamd64

[Models.NTamd64]
%CANON.SCSIDeviceDesc% = SCSI_SCANNER.NTamd64,CANON___DR-9050C________0
%CANON.SCSIDeviceDesc% = SCSI_SCANNER.NTamd64,CANON___DR-9050C________1
%CANON.SCSIDeviceDesc% = SCSI_SCANNER.NTamd64,CANON___DR-9050C________2
%CANON.SCSIDeviceDesc% = SCSI_SCANNER.NTamd64,CANON___DR-9050C________3
%CANON.USBDeviceDesc% = USB_SCANNER.NTamd64,USB\VID_1083&PID_1622


; ********** USB Section **********

[USB_SCANNER.NTamd64]
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=USB_SCAN.Events.NTamd64
DeviceData=USB_SCAN.DeviceData.NTamd64
AddReg=Usb.Scanner.AddReg.NTamd64
PropertyPages="DR905CPL.dll,EnumStiPropPages"
ICMProfiles="sRGB Color Space Profile.icm"

[USB_SCAN.DeviceData.NTamd64]
ISISDriverName="DR9050C.PXN"
TwainDS="Canon DR-9050C TWAIN"
Model=%CANON.USBDeviceDesc%
QueryNotification="DR905SVC.DLL"
MaxTransferBytes=16777215,1

[USB_SCAN.Events.NTamd64]
ScanButton="Scan Button",{AADF8531-9B29-4e93-8067-C8C186B0FEA3}, %LaunchApplication%
JobStartButton="Job Tool",{895DBEB0-1F4A-4756-ABFD-3218CF1F10A5},%LaunchJobApplication%


[USB_SCANNER.NTamd64.Services]
Include=sti.inf
Needs=STI.USBSection.Services


; ********** SCSI sections **********

[SCSI_SCANNER.NTamd64]
Include=sti.inf
Needs=STI.SCSISection
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=SCSI_SCAN.Events.NTamd64
DeviceData=SCSI_SCAN.DeviceData.NTamd64
AddReg=Scsi.Scanner.AddReg.NTamd64
PropertyPages="DR905CPL.dll,EnumStiPropPages"
DeviceSubType=0x0101
ICMProfiles="sRGB Color Space Profile.icm"

[SCSI_SCAN.DeviceData.NTamd64]
ISISDriverName="DR9050C.PXN"
TwainDS="Canon DR-9050C TWAIN"
Model=%CANON.SCSIDeviceDesc%
QueryNotification="DR905SVC.DLL"

[SCSI_SCAN.Events.NTamd64]
ScanButton="Scan Button",{AADF8531-9B29-4e93-8067-C8C186B0FEA3}, %LaunchApplication%
JobStartButton="Job Tool",{895DBEB0-1F4A-4756-ABFD-3218CF1F10A5},%LaunchJobApplication%


[SCSI_SCANNER.NTamd64.Services]
Include=sti.inf
Needs=STI.SCSISection.Services


; ********** Model-Generic add registry Section **********

[Scsi.Scanner.AddReg.NTamd64]
HKR,,HardwareConfig,1,2
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{7222EC61-956A-4bcf-B8D2-99A90B167594}"
HKCR,CLSID\{7222EC61-956A-4bcf-B8D2-99A90B167594},,,"Canon CeiSCSI64"
HKCR,CLSID\{7222EC61-956A-4bcf-B8D2-99A90B167594}\InProcServer32,,,%11%\ceiscs64.dll
HKCR,CLSID\{7222EC61-956A-4bcf-B8D2-99A90B167594}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"scsimap.sys,scsiscan.sys"

[Usb.Scanner.AddReg.NTamd64]
HKR,,HardwareConfig,1,4
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{DFDB3FF3-A518-4145-A404-D2C731EC4D63}"
HKCR,CLSID\{DFDB3FF3-A518-4145-A404-D2C731EC4D63},,,"Canon CeiUSB64"
HKCR,CLSID\{DFDB3FF3-A518-4145-A404-D2C731EC4D63}\InProcServer32,,,%11%\ceiusb64.dll
HKCR,CLSID\{DFDB3FF3-A518-4145-A404-D2C731EC4D63}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"usbscan.sys"


; ********** Source Disk Section **********

; the number is used in the SourceDisksFiles section
[SourceDisksNames]
; testing, change path below to path on media
1=%Disk Name%,,

; the number maps to the SourceDisksNames number
[SourceDisksFiles]

; ********** Strings **********

[Strings]
Provider="Canon Electronics Inc."
Mfg="CANON"
Disk Name="CANON DR-9050C Driver Disk"
CANON.SCSIDeviceDesc="CANON DR-9050C SCSI"
CANON.USBDeviceDesc="CANON DR-9050C USB"
LaunchApplication="*"
LaunchJobApplication="DR-9050C Job Tool"
