[Version]
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Provider%
DriverVer=05/08/2007,1.0.0.1
CatalogFile=CANODR201.cat

[DestinationDirs]
DefaultDestDir=11				; Win95,Win98 = \windows\system.  NT5 = \windows\system32
Usb.Scanner.CopySys32Files=10,system32\drivers  ; \windows\system32\drivers

[Manufacturer]
%Mfg%=Models

[Models]
%CANON.USBDeviceDesc% = USB_SCANNER,USB\VID_1083&PID_161B


; ********** USB Section **********

; Win98 model section
[USB_SCANNER]
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=USB_SCAN.Events
DeviceData=USB_SCAN.DeviceData
AddReg=Usb.Scanner.AddReg
CopyFiles=Usb.Scanner.CopyFiles,Usb.Scanner.CopySys32Files
PropertyPages="DR201CPL.dll,EnumStiPropPages"
;DeviceSubType=0x0105
ICMProfiles="sRGB Color Space Profile.icm"

; Win2000 model section
[USB_SCANNER.NT]
Include=sti.inf
Needs=STI.USBSection

SubClass=StillImage
DeviceType=1
Capabilities=3
Events=USB_SCAN.Events
DeviceData=USB_SCAN.DeviceData
AddReg=Usb.Scanner.AddReg.NT
CopyFiles=Usb.Scanner.CopyFiles.NT
PropertyPages="DR201CPL.dll,EnumStiPropPages"
;DeviceSubType=0x0105
;VendorSetup="Dr201svc.dll,EntryPointInst"
ICMProfiles="sRGB Color Space Profile.icm"

[USB_SCAN.DeviceData]
ISISDriverName="DR2010C.PXN"
TwainDS="Canon DR-2010C TWAIN"
Model=%CANON.USBDeviceDesc%
QueryNotification="DR201SVC.DLL"
MaxTransferBytes=4194304,1


[USB_SCAN.Events]
Button1="Button No.1",{0EDB75DD-C710-4dee-A76F-39724F12A0D4},%LaunchApplication%
Button2="Button No.2",{2EF082E2-5C4D-4bd0-8A91-49AD5798D7EE},%LaunchApplication%
Button3="Button No.3",{8EE5DA64-AF0A-4cc2-BDE5-690A908903CD},%LaunchApplication%
JobStartButton="Job Tool",{183085B1-6162-4858-8B40-BF43889FA6BA},%LaunchJobApplication%

[USB_SCANNER.NT.Services]
Include=sti.inf
Needs=STI.USBSection.Services


; ********** Model-Generic add registry and copy Section **********

; Win98 USB add registry section
[Usb.Scanner.AddReg]
HKR,,HardwareConfig,1,4
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{42B08D3F-3AC2-43c4-9455-E8264B18EB80}"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80},,,"Canon CeiUSB2"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,,,%11%\ceiusb2.dll
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"usbscan.sys"

; Win2000 USB add registry section
[Usb.Scanner.AddReg.NT]
HKR,,HardwareConfig,1,4
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{42B08D3F-3AC2-43c4-9455-E8264B18EB80}"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80},,,"Canon CeiUSB2"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,,,%11%\ceiusb2.dll
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"usbscan.sys"

; Win98 copy files section
[Usb.Scanner.CopyFiles]

; Win2000 copy files section
[Usb.Scanner.CopyFiles.NT]

; Only used by Win98
[Usb.Scanner.CopySys32Files]


; ********** Source Disk Section **********

; the number is used in the SourceDisksFiles section
[SourceDisksNames]
; testing, change path below to path on media
1=%Disk Name%,,

; the number maps to the SourceDisksNames number
[SourceDisksFiles]

; ********** Strings **********

[Strings]
Provider="Canon Electronics Inc."
Mfg="CANON"
Disk Name="CANON DR-2010C Driver Disk"
CANON.USBDeviceDesc="CANON DR-2010C USB"
LaunchApplication=*
LaunchJobApplication="DR-2010C Job Tool"


