; CANODR9K.INF  -- Canon DR-6080/7580/9080C Setup File
; Copyright (c) 2006 Canon Electronics Inc.

[Version]
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Provider%
DriverVer=11/06/2006,1.1.0.4
Catalogfile=CANODR9K.cat

[DestinationDirs]
DefaultDestDir=11				; Win95,Win98 = \windows\system.  NT5 = \windows\system32

[Manufacturer]
%Mfg%=Models

[Models]
%CANON_DR9080C.SCSIDeviceDesc% = CA9KSCSI,CANON___QUMA   _________B
%CANON_DR9080C.SCSIDeviceDesc% = CA9KSCSI,CANON___DR-9080C________0
%CANON_DR9080C.SCSIDeviceDesc% = CA9KSCSI,CANON___DR-9080C________1
%CANON_DR9080C.SCSIDeviceDesc% = CA9KSCSI,CANON___DR-9080C________2
%CANON_DR9080C.SCSIDeviceDesc% = CA9KSCSI,CANON___DR-9080C________3
%CANON_DR9080C.USBDeviceDesc% = CA9KUSB,USB\VID_04a9&PID_1603

; Win98 model section
[CA9KUSB]
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=CA9K.Events
DeviceData=CA9KUSB.DeviceData
AddReg=Usb.Scanner.AddReg
PropertyPages=%CA9K.PropertyPages%
ICMProfiles="sRGB Color Space Profile.icm"

; Win2000 model section
[CA9KUSB.NT]
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=CA9K.Events
DeviceData=CA9KUSB.DeviceData
AddReg=Usb.Scanner.AddReg.NT
PropertyPages=%CA9K.PropertyPages%
ICMProfiles="sRGB Color Space Profile.icm"

[CA9KUSB.NT.Services]
Include=sti.inf
Needs=STI.USBSection.Services


; ********** SCSI sections **********
; Win98 model section
[CA9KSCSI]
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=CA9K.Events
DeviceData=CA9KSCSI.DeviceData
AddReg=Scsi.Scanner.AddReg
PropertyPages=%CA9K.PropertyPages%
DeviceSubType=0x0101
ICMProfiles="sRGB Color Space Profile.icm"

; Win2000 model section
[CA9KSCSI.NT]
Include=sti.inf
Needs=STI.SCSISection
SubClass=StillImage
DeviceType=1
Capabilities=3
Events=CA9K.Events
DeviceData=CA9KSCSI.DeviceData
AddReg=Scsi.Scanner.AddReg.NT
PropertyPages=%CA9K.PropertyPages%
DeviceSubType=0x0101
ICMProfiles="sRGB Color Space Profile.icm"

[CA9KSCSI.NT.Services]
Include=sti.inf
Needs=STI.SCSISection.Services

; DeviceData
[CA9KUSB.DeviceData]
TwainDS=%CANON_DR9080C.TwainDSName%
ISISDriverName=%CA9K.ISISDriverName%
Model=%CANON_DR9080C.USBDeviceDesc%
QueryNotification="DR9KSVC.DLL"

[CA9KSCSI.DeviceData]
TwainDS=%CANON_DR9080C.TwainDSName%
ISISDriverName=%CA9K.ISISDriverName%
Model=%CANON_DR9080C.SCSIDeviceDesc%
QueryNotification="DR9KSVC.DLL"

; Events
[CA9K.Events]
ScanButton="Scan Button",{829A2E38-0F27-4389-A8A5-7735A76D9485}, *


; ********** Model-Generic add registry Section **********

; Win98 SCSI add registry section
[Scsi.Scanner.AddReg]
HKR,,HardwareConfig,1,2
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{9F33E1B0-5436-4dde-B1F8-214120CF8AA9}"
HKCR,CLSID\{9F33E1B0-5436-4dde-B1F8-214120CF8AA9},,,"Canon CeiSCSI"
HKCR,CLSID\{9F33E1B0-5436-4dde-B1F8-214120CF8AA9}\InProcServer32,,,%11%\ceiscsi.dll
HKCR,CLSID\{9F33E1B0-5436-4dde-B1F8-214120CF8AA9}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"scsimap.sys,scsiscan.sys"

; Win98 USB add registry section
[Usb.Scanner.AddReg]
HKR,,HardwareConfig,1,4
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{42B08D3F-3AC2-43c4-9455-E8264B18EB80}"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80},,,"Canon CeiUSB2"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,,,%11%\ceiusb2.dll
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"usbscan.sys"

; Win2000 SCSI add registry section
[Scsi.Scanner.AddReg.NT]
HKR,,HardwareConfig,1,2
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{9F33E1B0-5436-4dde-B1F8-214120CF8AA9}"
HKCR,CLSID\{9F33E1B0-5436-4dde-B1F8-214120CF8AA9},,,"Canon CeiSCSI"
HKCR,CLSID\{9F33E1B0-5436-4dde-B1F8-214120CF8AA9}\InProcServer32,,,%11%\ceiscsi.dll
HKCR,CLSID\{9F33E1B0-5436-4dde-B1F8-214120CF8AA9}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"scsimap.sys,scsiscan.sys"

; Win2000 USB add registry section
[Usb.Scanner.AddReg.NT]
HKR,,HardwareConfig,1,4
HKR,,DevLoader,,*NTKERN
HKR,,USDClass,,"{42B08D3F-3AC2-43c4-9455-E8264B18EB80}"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80},,,"Canon CeiUSB2"
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,,,%11%\ceiusb2.dll
HKCR,CLSID\{42B08D3F-3AC2-43c4-9455-E8264B18EB80}\InProcServer32,ThreadingModel,,"Apartment"
HKR,,NTMPDriver,,"usbscan.sys"


; ********** Strings **********

[Strings]
Provider="Canon Electronics Inc."
Mfg="CANON"
Disk Name="CANON DR-6080/7580/9080C Driver Disk"
CANON_DR9080C.SCSIDeviceDesc="CANON DR-9080C SCSI"
CANON_DR9080C.USBDeviceDesc="CANON DR-9080C USB"
CANON_DR9080C.TwainDSName="Canon DR-9080C TWAIN"
CA9K.ISISDriverName="DR9080C.PXN"
CA9K.PropertyPages="DR9KCPL.dll,EnumStiPropPages"
