;----------------------------------------------------------------------------
; CANON USB Adapter for MS
; CABULKM WDM (WithMPD)  Install INF   32bit  2000/XP/Vista/7, 98/Me
;
;                             8/June/2010
; Copyright (C) RATOC Systems,inc.
;
;;----------------------------------------------------------------------------
[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%RATOC%

;;LayoutFile=LAYOUT.INF
DriverVer=06/08/2010,3.8.0.0
Catalogfile=CANONx32.cat

;;[ControlFlags]
;;ExcludeFromSelect = *


;------------------------------------------------------------------------------
; Copy Files Section
;------------------------------------------------------------------------------
[CABULKM_WDM.files]
CABULKM.SYS

[CABULK_MPD.files]
CABULKRM.MPD


[CABULK_2K.files]
CABLKM2.SYS
CABLKRM2.SYS

[SourceDisksNames]
1="CANON USB Adapter for MS Installation Disk",,

[SourceDisksFiles]
CABULKM.SYS = 1
CABULKRM.mpd = 1
CABLKM2.SYS = 1
CABLKRM2.sys = 1
CABULKM.inf = 1


[DestinationDirs]
CABULKM_WDM.files = 10,System32\Drivers
CABULK_MPD.files = 12		; \<WINDIR>\SYSTEM\IOSUBSYS
CABULK_2K.files = 10,System32\Drivers




; ----------------------------------------
; Manufacturer Sections
[Manufacturer]
%RATOC%=RATOC

[RATOC]
%CABULK.DeviceDesc% = CABULKM_WDM, USB\VID_1083&PID_1615

%CABULK.DeviceDesc% = CABULKM_WDM, USB\VID_0584&PID_0305	;; U2SCX-LVD
%CABULK.DeviceDesc% = CABULKM_WDM, USB\VID_0584&PID_0051	;; MR-01

[CABULKM_WDM]
CopyFiles = CABULKM_WDM.files, CABULK_MPD.files
AddReg=CABULKM_WDM.AddReg

[CABULKM_WDM.addreg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,CABULKM.SYS
HKLM,"System\Currentcontrolset\Services\CABULKM\Parameters","DebugLevel",0x10001,0



[CABULKM_WDM.NT]
CopyFiles = CABULK_2K.files
AddReg=CABULKM_WDM2K.AddReg

[CABULKM_WDM.NT.Services]
Addservice = CABLKM2, 0x00000002, CABULKM_WDM.AddService

[CABULKM_WDM.AddService]
DisplayName    = %CABULK.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\CABLKM2.SYS

[CABULKM_WDM2K.AddReg]
HKLM,"System\Currentcontrolset\Services\CABLKM2\Parameters","DebugLevel",0x10001,0
HKLM,"System\Currentcontrolset\Services\CABLKM2\Parameters","MaximumTransferSize",0x10001,0x40000



[CABULKM_WDM.addreg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,CABULKM.SYS
HKLM,"System\Currentcontrolset\Services\CABULKM\Parameters","DebugLevel",0x10001,0
HKLM,"System\Currentcontrolset\Services\CABULKM\Parameters","MaximumTransferSize",0x10001,0x40000


;---------------------------------------------------------------;

[Strings]
RATOC="Canon Electronics Inc."
RATOC2="Canon Electronics Inc."
MfgName="Canon Electronics Inc."
CABULK.DeviceDesc="CANON USB Adapter for MS WDM (withMPD)"
CABULK.SvcDesc="CANON USB Adapter for MS WDM driver"

